AIR COMPRESSOR INSPECTION CHECKLIST

|  |  |
| --- | --- |
| **EVENT:** | **YEAR:**  |
| NOTEDo not "tick". Write OK or use the number of the specific deviation given in the legend. |
| **LEGEND****Indicate the “action” to be taken by number as indicated under “Corrective Action” below,**  specify the exact repairs to be done on a works request or job card |
| 1. Dirty – oil/dust etc. on compressor
2. Oil leaks on compressor
3. V-belt drive not guarded
4. Guard does not cover back side
5. No red line on meter dial face
6. Safety valve not locked or sealed or not calibrated
7. Drain valve not accessible
8. Compressor not numbered or identified
9. Manufacturers plate not displayed or visible
10. Compressor due for pressure test (3-yearly to 1,25 x MPOP)
11. Electric cord/plug not in good state of repair

13 Other – specify |
| **ID NO** | LOCATION | **1ST QUARTER** | **2ND QUARTER** | **3RD QUARTER** | **4TH QUARTER** |
| **Check** | **Action** | **Check** | **Action** | **Check** | **Action** | **Check** | **Action** |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  |  |  |  |  |
| DATE INSPECTED |  |  |  |  |
| INSPECTOR’S INITIALS |  |  |  |  |
| AUDIT/SPOT CHECK |  |  |  |  |  |  |  |  |